{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H"]
[]
[]
[]
[]
["","","","","","FCAHG71HVEB","FCAHG100HVEB","FCAHG125HVEB","FCAHG140HVEB"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","6.80","9.50","12.10","13.40"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","7.50","10.8","13.5","15.5"]
["Opláštenie","Materiál","","","","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","288","288","288","288"]
["","","","Šírka","mm","840","840","840","840"]
["","","","Hĺbka","mm","840","840","840","840"]
["Hmotnosť","Jednotka","","","kg","25","25","25","25"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","23.6","32.2","34.4","34.4"]
["","","","Stredný","m³/min","18.8","25.7","27.3","27.3"]
["","","","Nízka","m³/min","13.7","19.1","21.2","21.2"]
["","","Kúrenie","Vysoké","m³/min","23.6","30.8","32.1","32.1"]
["","","Vykurovanie","Stredný","m³/min","18.8","24.6","25.5","25.5"]
["","","Kúrenie","Nízka","m³/min","13.7","18.3","19.7","19.7"]
["Akustický výkon","Chladenie","","","dBA","53","61","61","61"]
["","Vykurovanie","","","dBA","53","61","61","61"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","36","44","45","45"]
["","","","Stredný","dBA","33","39","40","41"]
["","","","Nízka","dBA","29","33","35","37"]
["","Kúrenie","","Vysoké","dBA","36","44","45","45"]
["","Vykurovanie","","Stredný","dBA","33","39","40","41"]
["","Kúrenie","","Nízka","dBA","29","33","35","37"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","9.52","9.52","9.52"]
["","Plyn","","OD","mm","15.9","15.9","15.9","15.9"]
["","Odvod kondenzátu","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dekoračný panel","Model","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Vonkajšie rozmery","","Výška","mm","65","65","65","65"]
["","","","Šírka","mm","950","950","950","950"]
["","","","Hĺbka","mm","950","950","950","950"]
["","Hmotnosť","","","kg","5.5","5.5","5.5","5.5"]
["Dekoračný panel 2","Model","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Vonkajšie rozmery","","Výška","mm","148","148","148","148"]
["","","","Šírka","mm","950","950","950","950"]
["","","","Hĺbka","mm","950","950","950","950"]
["","Hmotnosť","","","kg","10.3","10.3","10.3","10.3"]
["Dekoračný panel 3","Model","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Vonkajšie rozmery","","Výška","mm","106","106","106","106"]
["","","","Šírka","mm","950","950","950","950"]
["","","","Hĺbka","mm","950","950","950","950"]
["","Hmotnosť","","","kg","6.5","6.5","6.5","6.5"]
["Riadiace systémy","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1"]
["","Clamps","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation guide","","","","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2"]
["","Screws","","","","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~"]
["Zdroj napájania","Zdroj napájania-=-Frekvencia","","Frekvencia","","50/60","50/60","50/60","50/60"]
["","Zdroj napájania-=-Napätie","","Napätie","","220-240/220","220-240/220","220-240/220","220-240/220"]