{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / AZQS100B7Y1B UK","FCQG125FVEB / AZQS125B7Y1B UK","FCQG140FVEB / AZQS140B7Y1B UK"]
["Chladiaci výkon","Men.","","kW","9.5","12.1","13.0"]
["Chladenie","SEER","","","5.50"]
["","Ročná spotreba energie","","kWh/a","605"]
["","Výkon","P návrh","kW","9.50"]
["","Trieda energetickej účinnosti","","","A"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","7.60"]
["","SCOP/A","","","3.85"]
["","Trieda energetickej účinnosti","","","A"]
["","Ročná spotreba energie","","kWh/a","2,764"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","1,480","1,952","2,313"]
["","EER","","","3.21","3.10","2.81"]
["","COP","","","3.50","3.41","3.30"]
["","Smernica o energetickom označovaní","Chladenie","","A","B"]
["","","Vykurovanie","","B","B"]
["Vykurovací výkon","Men.","","kW","10.8","13.5","15.5"]
["Poznámky","","","","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES"]
["","","","","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825"]
["","","","","(3) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(3) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(3) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]