{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":21,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQG71L9V1B","FCQG71FVEB / RZQG71L9V1B","FCQG35FVEB / FCQG35FVEB / RZQG71L9V1B","FCQG100FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG100L9V1B","FCQG140FVEB / RZQG100L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L9V1B","FCQG125FVEB / RZQG125L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L9V1B","FCQG71FVEB / FCQG71FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG125L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L9V1B","FCQG60FVEB / FCQG60FVEB / RZQG125L9V1B","FCQG140FVEB / RZQG140L9V1B"]
["Chladiaci výkon","Men.","","kW","","6.8","","9.5","","","","","","","12.0","","","","","","13.4"]
["Chladenie priestoru","SEER","","","6.80","6.72","5.10","6.80","5.10","5.10","5.10","6.80","5.10","5.10","6.00","5.10","5.10","6.00","5.10","5.10"]
["","Ročná spotreba energie","","kWh/a","350","355","467","489","652","652","652","489","652","652","700","824","824","700","824","824"]
["","Výkon","P návrh","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Trieda energetickej účinnosti","","","A++","A++","B","A++","B","B","B","A++","B","B","A+","B","B","A+","B","B"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","6.33","6.33","6.00","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.66","12.71","12.71","12.66","12.71","12.71"]
["","SCOP/A","","","4.20","4.20","3.80","4.61","3.80","3.80","3.80","4.61","3.80","3.80","4.10","3.80","3.80","4.10","3.80","3.80"]
["","Trieda energetickej účinnosti","","","A+","A+","A","A++","A","A","A","A++","A","A","A+","A","A","A+","A","A"]
["","Ročná spotreba energie","","kWh/a","2,110","2,110","2,211","3,432","4,164","4,164","4,164","3,432","4,164","4,164","4,323","4,683","4,683","4,323","4,683","4,683"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","1,005","","1,225","","","","","","","1,610"]
["","EER","","","","3.39","","3.87","","","","","","","3.73","","","","","","3.21"]
["","COP","","","","3.97","","4.15","","","","","","","3.63","","","","","","3.61"]
["","Smernica o energetickom označovaní","Chladenie","","","A","","A","","","","","","","A"]
["","","Vykurovanie","","","A","","A","","","","","","","A"]
["Vykurovací výkon","Men.","","kW","","7.5","","10.8","","","","","","","13.5","","","","","","15.5"]
["Poznámky","","","","","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","","","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]
["","","","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]