{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQG71L9V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L9V1B","FCQG140FVEB / RZQG100L9V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L9V1B"]
["Chladenie priestoru","SEER","","","6.80","5.10","6.80","5.10"]
["","Ročná spotreba energie","","kWh/a","350","652","489","824"]
["","Výkon","P návrh","kW","6.80","9.50","9.50","12.00"]
["","Trieda energetickej účinnosti","","","A++","B","A++","B"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","6.33","11.30","11.30","12.71"]
["","SCOP/A","","","4.20","3.80","4.61","3.80"]
["","Trieda energetickej účinnosti","","","A+","A","A++","A"]
["","Ročná spotreba energie","","kWh/a","2,110","4,164","3,432","4,683"]