{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQG71L9V1B","FCQHG71FVEB / RZQG71L9V1B","FCQHG100FVEB / RZQG100L9V1B","FCQHG71FVEB / FCQHG71FVEB / RZQG100L9V1B","FCQHG140FVEB / RZQG100L9V1B","FCQHG125FVEB / RZQG125L9V1B","FCQHG71FVEB / FCQHG71FVEB / RZQG125L9V1B","FCQHG140FVEB / RZQG125L9V1B","FCQHG140FVEB / RZQG140L9V1B"]
["Chladiaci výkon","Men.","","kW","","6.8","9.5","","","12.0","","","13.4"]
["Chladenie","SEER","","","7.00","6.91","7.00","5.10","7.00","6.61","5.10","6.61"]
["","Ročná spotreba energie","","kWh/rok","340","345","475","652","475","636","824","636"]
["","Výkon","P návrh","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Trieda energetickej účinnosti","","","A++","A++","A++","B","A++","A++","B","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","7.60","7.60","11.30","11.30","11.30","12.66","12.71","12.66"]
["","SCOP/A","","","4.54","4.54","4.80","3.80","4.80","4.63","3.80","4.63"]
["","Trieda energetickej účinnosti","","","A+","A+","A++","A","A++","A++","A","A++"]
["","Ročná spotreba energie","","kWh/rok","2,344","2,344","3,296","4,164","3,296","3,829","4,683","3,829"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","830","1,075","","","1,500"]
["","EER","","","","4.09","4.42","","","4.00","","","3.35"]
["","COP","","","","4.80","4.99","","","4.40","","","4.12"]
["","Smernica o energetickom označovaní","Chladenie","","","A","A","","","A"]
["","","Vykurovanie","","","A","A","","","A"]
["Vykurovací výkon","Men.","","kW","","7.5","10.8","","","13.5","","","15.5"]
["Poznámky","","","","","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]