{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RQ-BW1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RQ125B8W1B"]
["Chladiaci výkon","Men.","","kW","12.2 (3)"]
["Nominálna účinnosť","EER","","","2.70"]
["","Annual energy consumption","","kWh","2,260"]
["","COP","","","3.30"]
["","Smernica o energetickom označovaní","Chladenie","","D"]
["","","Vykurovanie","","C"]
["Vykurovací výkon","Men.","","kW","14.5 (5)"]
["Poznámky","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 5m; výškový rozdiel: 0m"]
["","","","","(2) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","(3) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m (horizontálne); úrovňového rozdielu: 0m"]
["","","","","(4) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m; výškový rozdiel: 0m"]
["","","","","(5) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]