{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","12.10","19.00","22.00"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","13.50","22.4","24.0"]
["Opláštenie","Farba","","","","Bez náteru","Bez náteru","Bez náteru"]
["","Materiál","","","","Pozinkovaná oceľ","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","300","470","470"]
["","","","Šírka","mm","1,400","1,490","1,490"]
["","","","Hĺbka","mm","700","1,100","1,100"]
["Hmotnosť","Jednotka","","","kg","45","104","115"]
["Požadovaný priestor pod stropom >","mm","","","","350"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","39.0","64.0","69.0"]
["","","","Stredný","m³/min","","50","56"]
["","","","Nízka","m³/min","28.0","36.0","43.0"]
["","","Kúrenie","Vysoké","m³/min","39.0","64.0","69.0"]
["","","","Stredný","m³/min","","50.0","56.0"]
["","","","Nízka","m³/min","28.0","36.0","43.0"]
["","Externý statický tlak","","Vysoký","Pa","200","250","250"]
["","","","Nom. ot.","Pa","50","62","62"]
["Sound power level","Chladenie","","","dBA","66","69.0","71.0"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","40","43.0","44.0"]
["","","","Stredný","dBA","","39.0","40.0"]
["","","","Nízka","dBA","33","36.0","37.0"]
["","Kúrenie","","Vysoké","dBA","40","43.0","44.0"]
["","","","Stredný","dBA","","39.0","40.0"]
["","","","Nízka","dBA","33","36.0","37.0"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","9.52","9.52"]
["","Plyn","","OD","mm","15.90","19.1","22.2"]
["","Vypúšťanie","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Výška odsávania","mm","","","","625"]
["Dekoračný panel","Model","","","","BYBS125DJW1"]
["","Farba","","","","Biela (10Y9/0,5)"]
["","Vonkajšie rozmery","","Výška","mm","55"]
["","","","Šírka","mm","1,500"]
["","","","Hĺbka","mm","500"]
["","Hmotnosť","","","kg","6.5"]
["Riadiace systémy","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Štandardné príslušenstvo","Skrutky","","","","16","2","2"]
["","Podložka","","","","8","12","12"]
["","Pás hadice","","","","1"]
["","Vypúšťacia hadica","","","","1"]
["","Všeobecné bezpečnostné opatrenia","","","","1","1","1"]
["","Návod na montáž a prevádzku","","","","1","1","1"]
["","Vodič pre bežné napájanie","","","","2"]
["","Tesniaci materiál (odvodová hadica)","","","","1"]
["","Tesniaci materiál","","","","2"]
["","Tepelná izolačná rúrka (kvapalina)","","","","1"]
["","Tepelná izolačná rúrka (plyn)","","","","1"]
["Power supply","Názov","","","","","VE","VE"]
["","Fáza","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50/60","50/60","50/60"]
["","Napätie","","","V","220-240/220","220-240/220","220-240/220"]
["Poznámky","","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["Štandardné príslušenstvo","Návod na prevádzku","","","","","1","1"]
["","Návod na montáž","","","","","1","1"]
["","Pripájanie plynové potrubie","","","","","1","1"]
["","Materiál svorky vodiča","","","","","1","1"]
["","Pružinová podložka","","","","","2","2"]
["","Skrutka + podložka","","","","","45","45"]
["","Skrutka so šesťhrannou hlavou a podložkou","","","","","49","49"]
["","Skrutka so šesťhrannou hlavou","","","","","2","2"]
["","Plochá podložka","","","","","8","8"]