{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","35.0","35.0"]
["","","","Nízka","dBA","29.0","29.0"]
["","Chladenie","","Nízka","dBA","28.0","28.0"]
["","","","Vysoké","dBA","35.0","35.0"]
["Štandardné príslušenstvo","Návod na montáž a prevádzku","","","","1","1"]
["","Sací vzduchový filter","","","","1","1"]
["Riadiace systémy","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Pripojenia potrubí","Liquid","","OD","mm","6.35"]
["","Plyn","","OD","mm","9.52"]
["","Vypúšťanie","","","","27.2"]
["Akustický výkon","Chladenie","","","dBA","55","55"]
["","Vykurovanie","","","dBA","55","55"]
["Rozmery","Jednotka","","Šírka","mm","652","652"]
["","","","Depth","mm","502","502"]
["","","","Výška","mm","230","230"]
["Opláštenie","Material","","","","Pozinkovaná oceľ s nízkym obsahom uhlíka","Pozinkovaná oceľ s nízkym obsahom uhlíka"]
["Hmotnosť","Jednotka","","","kg","17.0","17.0"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","","6.95"]
["","","","Nízka","m³/min","","5.20"]
["","","Chladenie","Nízka","m³/min","","5.20"]
["","","","Vysoké","m³/min","","6.50"]
["Power supply","Fáza","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Názov","","","","V1","V1"]
["","Napätie","","","V","230","230 +/-10%"]
["Poznámky","","","","","(1) - Hodnoty hluku sa merajú v čiastočne bezodrazovej miestnosti.","(1) - Hodnoty hluku sa merajú v čiastočne bezodrazovej miestnosti."]
["","","","","","(2) - Hladina akustického tlaku predstavuje relatívnu hodnotu závislú od vzdialenosti a akustiky. Podrobnosti si prosím pozrite vo výkresoch hladiny hluku.","(2) - Hladina akustického tlaku predstavuje relatívnu hodnotu závislú od vzdialenosti a akustiky. Podrobnosti si prosím pozrite vo výkresoch hladiny hluku."]
["","","","","","(3) - Hladina zvuku je absolútna hodnota, ktorá uvádza výkon, ktorý generuje zdroj zvuku.","(3) - Hladina zvuku je absolútna hodnota, ktorá uvádza výkon, ktorý generuje zdroj zvuku."]
["Pripojenia potrubí","Liquid","","OD","mm","","6.35"]
["","Plyn","","OD","mm","","9.52"]
["","Vypúšťanie","","","","","27.2"]