{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-DV1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D7V1B"]
["Chladiaci výkon","Men.","","kW","12.5 (1)"]
["Pripojenia potrubí","Kvapalný","OD","mm","9.52"]
["","Gas","OD","mm","15.9"]
["","Drain","OD","mm","26"]
["Nominálna účinnosť","Annual energy consumption","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Smernica o energetickom označovaní","Chladenie","","B"]
["","","Vykurovanie","","A"]
["Vykurovací výkon","Men.","","kW","14.0 (2)"]
["Poznámky","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 5m; výškový rozdiel: 0m"]
["","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m; výškový rozdiel: 0m"]
["","","","","(3) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]