{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB","FDQ125C5VEB"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","40","40"]
["","","Nízka","dBA","33","33"]
["","Chladenie","Nízka","dBA","33","33"]
["","","Vysoké","dBA","40","40"]
["Riadiace systémy","Káblový diaľkový ovládač","","","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D528","BRC1D52, BRC1E53A, BRC1E53B, BRC1E53C"]
["","Infrared remote control","","","BRC4C65","BRC4C65"]
["Chladiaci výkon","Celkový výkon","Men.","kW","12.5","12.5 (1)"]
["Pripojenia potrubia","Kvapalina","OD","mm","9.52","9.52"]
["","Plyn","OD","mm","15.9","15.9"]
["","Vypúšťanie","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Power input","Chladenie","Men.","kW","","0.35"]
["","Kúrenie","Men.","kW","","0.35"]
["Požadovaný priestor pod stropom >","mm","","","350","350"]
["Sound power level","Chladenie","","dBA","66","66"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","1,400","1,400"]
["","","Hĺbka","mm","700","700"]
["","","Výška","mm","300","300"]
["Opláštenie","Materiál","","","Pozinkovaná oceľ"]
["","Farba","","","Not painted","Nenatretý (pozinkovaný)"]
["Hmotnosť","Jednotka","","kg","45","45"]
["Ventilátor","Atmosférický tlak vonkajšieho prostredia","Vysoký","Pa","200","200"]
["","","Nom. ot.","Pa","50","50"]
["Výška odsávania","mm","","","625","625"]
["Dekoračný panel","Hmotnosť","","kg","6.5","6.5"]
["","Model","","","BYBS125DJW1","BYBS125DJW1"]
["","Vonkajšie rozmery","Výška","mm","55","55"]
["","","Hĺbka","mm","500","500"]
["","","Šírka","mm","1,500","1,500"]
["","Farba","","","Biela (10Y9/0,5)","Biela (10Y9/0,5)"]
["Vykurovací výkon","Celkový výkon","Nom. ot.","kW","14.0","14.0 (2)"]
["Power supply","Fáza","","","1~","1~"]
["","Frekvencia","","Hz","50/60","50/60"]
["","Názov","","","VE","VE"]
["","Napätie","","V","220-240/220","220-240/220"]
["Poznámky","","","","(1) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m","(1) - Chladenie: vnútorná teplota 27°CDB, 19,0°CWB; vonkajšia teplota 35°CDB; príslušná dĺžka potrubia: 7,5 m; prevýšenie: 0 m"]
["","","","","(2) - Výkony predstavujú čisté výkony vrátane odpočítania na chladenie (okrem vykurovania) motora izbového ventilátora.","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]
["","","","","(3) - Hodnoty akustického tlaku sú určené pre jednotku inštalovanú so zadným nasávaním.","(3) - Výkony predstavujú čisté výkony vrátane odpočítania na chladenie (okrem vykurovania) motora izbového ventilátora."]
["","","","","(4) - Kategória jednotky PED: vylúčená z rozsahu PED kvôli článku 1, položka 3.6 Smernice 97/23/ES","(4) - Hodnoty akustického tlaku sú určené pre jednotku inštalovanú so zadným nasávaním."]
["","","","","(5) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m (horizontálne); úrovňového rozdielu: 0m","(5) - Kategória jednotky PED: vylúčená z rozsahu PED kvôli článku 1, položka 3.6 Smernice 97/23/ES"]