{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F"]
[]
[]
[]
[]
["","","","","FDXM25F2V1B","FDXM35F2V1B","FDXM50F2V1B","FDXM60F2V1B"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","35","35","38","38"]
["","","Nízka","dBA","27","27","30","30"]
["","Chladenie","Nízka","dBA","27","27","30","30"]
["","","Vysoké","dBA","35","35","38","38"]
["","","Men.","dBA","33","33","36","36"]
["","Chladenie","Men.","dBA","33","33","36","35"]
["Riadiace systémy","Wired remote control","","","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Pripojenia potrubí","Kvapalina","OD","mm","6.35","6.35","6.35","6.35"]
["","Plyn","OD","mm","9.5","9.5","12.7","12.7"]
["","Vypúšťanie","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Príkon","Chladenie","Men.","kW","0.036","0.036","0.060","0.060"]
["","Kúrenie","Men.","kW","0.036","0.036","0.060","0.060"]
["Sound power level","Chladenie","","dBA","53","53","55","56"]
["","Vykurovanie","","dBA","53","53","55","56"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","750","750","1,150","1,150"]
["","","Hĺbka","mm","620","620","620","620"]
["","","Výška","mm","200","200","200","200"]
["Hmotnosť","Jednotka","","kg","21","21","30","30"]
["Ventilátor","Externý statický tlak","Nom. ot.","Pa","30","30","40","40"]
["Power supply","Fáza","","","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50","50","50","50"]
["","Názov","","","V1","V1","V1","V1"]
["","Napätie","","V","230","230","220-240","220-240"]