{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Chladiaci výkon","Min.","","kW","","1.70"]
["","Men.","","kW","","6.00"]
["","Max.","","kW","","6.50"]
["Vykurovací výkon","Min.","","kW","","1.70"]
["","Men.","","kW","","7.00"]
["","Max.","","kW","","7.10"]
["Nominálna účinnosť","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Annual energy consumption","","kWh","","1,024"]
["","Smernica o energetickom označovaní","Chladenie","","","C"]
["","","Vykurovanie","","","C"]
["Chladenie","Trieda energetickej účinnosti","","","","A"]
["","Výkon","P návrh","kW","","6.00"]
["","SEER","","","","5.56"]
["","Ročná spotreba energie","","kWh/a","","378"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","A"]
["","Výkon","P návrh","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Ročná spotreba energie","","kWh/a","","1,693"]
["Poznámky","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Chladiaci výkon","Min.","","kW","1.70"]
["","Men.","","kW","5.00"]
["","Max.","","kW","5.30"]
["Vykurovací výkon","Min.","","kW","1.70"]
["","Men.","","kW","5.80"]
["","Max.","","kW","6.00"]
["Nominálna účinnosť","EER","","","3.06"]
["","COP","","","3.10"]
["","Ročná spotreba energie","","kWh","816"]
["","Smernica o energetickom označovaní","Chladenie","","B"]
["","","Vykurovanie","","D"]
["Chladenie","Trieda energetickej účinnosti","","","A+"]
["","Výkon","P návrh","kW","5.00"]
["","SEER","","","5.77"]
["","Ročná spotreba energie","","kWh/a","303"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A"]
["","Výkon","P návrh","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh Vykurovací výkon pri -10°","","kW","3.55"]
["","Ročná spotreba energie","","kWh/a","1424"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D"]