{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXS50L2V1B","FDXM60F3V1B9 / RXS60L2V1B"]
["Chladiaci výkon","Min.","","kW","1.70","1.70"]
["","Max.","","kW","5.30","6.50"]
["","Men.","","kW","5.00","6.00"]
["Pripojenia potrubia","Kvapalina","OD","mm","6.35","6.35"]
["","Plyn","OD","mm","12.70","12.70"]
["","Vypúšťanie","OD","mm","VP20 (Externý priemer 26, Interný priemer 20)","VP20 (Externý priemer 26, Interný priemer 20)"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","825","1,030"]
["","EER","","","3.03","2.91"]
["","COP","","","3.10","3.21"]
["","Smernica o energetickom označovaní","Chladenie","","B","C"]
["","","Vykurovanie","","D","C"]
["Vykurovací výkon","Men.","","kW","5.80","7.00"]
["","Min.","","kW","1.70","1.70"]
["","Max.","","kW","6.00","8.00"]
["Poznámky","","","","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["","","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(4) - Elektrické údaje nájdete v samostatných nákresoch","(4) - Elektrické údaje nájdete v samostatných nákresoch"]