{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG125L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG125L8Y1B","FDXM60F3V1B9 / FDXM60F3V1B9 / RZQG125L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG71L8Y1B"]
["Chladiaci výkon","Men.","","kW","","","","","","","","6.80","6.80","6.80"]
["Chladenie","SEER","","","","","","","","","","4.80","4.80","4.80"]
["","Ročná spotreba energie","","kWh/a","","","","","","","","496","496","496"]
["","Výkon","P návrh","kW","","","","","","","","6.80","6.80","6.80"]
["","Trieda energetickej účinnosti","","","","","","","","","","B","B","B"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Trieda energetickej účinnosti","","","","","","","","","","A","A","A"]
["","Ročná spotreba energie","","kWh/a","","","","","","","","2,211","2,211","2,211"]
["Nominálna účinnosť","EER","","","","","","","","","","3.06","3.06","3.06"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Poznámky","","","","","","","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","","","","","","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","","","","","","","(4) - Elektrické údaje nájdete v samostatných nákresoch"]