{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Vstup napájania","Chladenie","","Men.","kW","0.036","0.036","0.060","0.060"]
["","Kúrenie","","Men.","kW","0.036","0.036","0.060","0.060"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","200","200","200","200"]
["","","","Šírka","mm","750","750","1150","1150"]
["","","","Hĺbka","mm","620","620","620","620"]
["Hmotnosť","Jednotka","","","kg","21","21","28","28"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","8.7","8.7","15.8","16.0"]
["","","","Stredný","m³/min","8.0","8.0","14.6","14.8"]
["","","","Nízka","m³/min","7.3","7.3","13.3","13.5"]
["","","Kúrenie","Vysoké","m³/min","8.7","8.7","15.8","16.0"]
["","","Vykurovanie","Stredný","m³/min","8.0","8.0","14.6","14.8"]
["","","Kúrenie","Nízka","m³/min","7.3","7.3","13.3","13.5"]
["","Externý statický tlak","","Nom. ot.","Pa","30","30","40","40"]
["Akustický výkon","Chladenie","","","dBA","53.0","53.0","55.0","56.0"]
["","Vykurovanie","","","dBA","53.0","53.0","55.0","56.0"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","35.0","35.0","38.0","38.0"]
["","","","Stredný","dBA","33.0","33.0","35.0","35.0"]
["","","","Nízka","dBA","27.0","27.0","30.0","30.0"]
["","Kúrenie","","Vysoké","dBA","35.0","35.0","38.0","38.0"]
["","Vykurovanie","","Stredný","dBA","33.0","33.0","35.0","35.0"]
["","Kúrenie","","Nízka","dBA","27.0","27.0","30.0","30.0"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35","6.35","6.35"]
["","Plyn","","OD","mm","9.50","9.50","12.70","12.70"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Clamp metal","","","","1","1","1","1"]
["","Clamps","","","","6","6","6","6"]
["","Drain hose","","","","1","1","1","1"]
["","Vzduchový filter","","","","1","1","1","1"]
["","Insulation for fitting","","","","1","1","1","1"]
["","Screws for duct flanges","","","","1","1","1","1"]
["","Sealing material","","","","2","2","2","2"]
["","Sealing pad","","","","1","1","1","1"]
["","Washer fixing plate","","","","4","4","4","4"]
["Rozsah energetickej účinnosti","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napájanie","Fáza","","","","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch"]