{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Hladina akust. tlaku","Kúrenie","","Vysoké","dBA","35.0","35.0","","38.0"]
["","","","Stredný","dBA","33.0","33.0","","35.0"]
["","","","Nízka","dBA","27.0","27.0","","30.0"]
["","Chladenie","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Nízka","dBA","27.0","27.0","","30.0"]
["","","","Vysoké","dBA","35.0","35.0","","38.0"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","1","","1"]
["","Návod na prevádzku","","","","1","1","","1"]
["","Izolácia príslušenstva","","","","1","1","","1"]
["","Tesniaca podložka","","","","1","1","","1"]
["","Kovová svorka","","","","1","1","","1"]
["","Vypúšťacia hadica","","","","1","1","","1"]
["","Podložka pre držiak ramena","","","","8","8","","8"]
["","Tesniaci materiál","","","","2","2","","2"]
["","Svorky","","","","6","6","","6"]
["","Upevňovacia doska podložky","","","","4","4","","4"]
["","Skrutky na príruby potrubia","","","","1","1","","1"]
["","Vzduchový filter","","","","1","1","","1"]
["Pripojenia potrubí","Kvapalný","","OD","mm","6.35","6.35","","6.35"]
["","Plyn","","OD","mm","9.50","9.50","","12.70"]
["","Vypúšťanie","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Vstup napájania","Chladenie","","Men.","kW","0.036","0.036","","0.060"]
["","Kúrenie","","Men.","kW","0.036","0.036","","0.060"]
["Úroveň akustického výkonu","Chladenie","","","dBA","53.0","53.0","","56.0"]
["","Vykurovanie","","","dBA","53.0","53.0","","56.0"]
["Rozmery","Jednotka","","Šírka","mm","750","750","","1,150"]
["","","","Hĺbka","mm","620","620","","620"]
["","","","Výška","mm","200","200","","200"]
["Hmotnosť","Jednotka","","","kg","21","21","","28"]
["Ventilátor","Atmosférický tlak vonkajšieho prostredia","","Men.","Pa","30","30","","40"]
["","Prietok vzduchu","Kúrenie","Vysoké","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Nízka","m³/min","7.3","7.3","","13.5"]
["","","Cooling","Nízka","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Vysoké","m³/min","8.7","8.7","","16.0"]
["Power supply","Fáza","","","","1~","1~","","1~"]
["","Frekvencia","","","Hz","50","50","","50"]
["","Napätie","","","V","220-240","220-240","","220-240"]
["Poznámky","","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch","","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["Vstup napájania","Chladenie","","Men.","kW","","","0.060"]
["","Kúrenie","","Men.","kW","","","0.060"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","200"]
["","","","Šírka","mm","","","1150"]
["","","","Hĺbka","mm","","","620"]
["Hmotnosť","Jednotka","","","kg","","","28"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","","15.8"]
["","","","Stredný","m³/min","","","14.6"]
["","","","Nízka","m³/min","","","13.3"]
["","","Kúrenie","Vysoké","m³/min","","","15.8"]
["","","Vykurovanie","Stredný","m³/min","","","14.6"]
["","","Kúrenie","Nízka","m³/min","","","13.3"]
["","Externý statický tlak","","Nom. ot.","Pa","","","40"]
["Akustický výkon","Chladenie","","","dBA","","","55.0"]
["","Vykurovanie","","","dBA","","","55.0"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","","38.0"]
["","","","Stredný","dBA","","","35.0"]
["","","","Nízka","dBA","","","30.0"]
["","Kúrenie","","Vysoké","dBA","","","38.0"]
["","Vykurovanie","","Stredný","dBA","","","35.0"]
["","Kúrenie","","Nízka","dBA","","","30.0"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","","6.35"]
["","Plyn","","OD","mm","","","12.70"]
["","Odvod kondenzátu","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Štandardné príslušenstvo","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Air filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Napájanie","Fáza","","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","50"]
["","Napätie","","","V","","","220-240"]