{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25L3V1B","FDXS35F2VEB / RXS35L3V1B"]
["Chladiaci výkon","Min.","","kW","1.3","1.4"]
["","Max.","","kW","3.0","3.8"]
["","Men.","","kW","2.4 (2)","3.4 (2)"]
["Pripojenia potrubia","Liquid","OD","mm","6.35","6.35"]
["","Plyn","OD","mm","9.5","9.5"]
["","Vypúšťanie","OD","mm","VP20 (Externý priemer 26, Interný priemer 20)","VP20 (Externý priemer 26, Interný priemer 20)"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","321","574"]
["","EER","","","3.74 (1)","2.96 (1)"]
["","COP","","","4.00 (1)","3.48 (1)"]
["","Smernica o energetickom označovaní","Chladenie","","A","B"]
["","","Vykurovanie","","A","A"]
["Vykurovací výkon","Men.","","kW","3.2 (2)","4.0 (2)"]
["","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.5","5.0"]
["Poznámky","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]