{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXM25M3V1B9","FFA35A2VEB / RXM35M3V1B9","FFA50A2VEB / RXM50M3V1B9","FFA60A2VEB / RXM60M3V1B9"]
["Chladiaci výkon","Men.","","kW","2.50","3.40"]
["Chladenie","SEER","","","6.17","6.38"]
["","Ročná spotreba energie","","kWh/rok","142","186"]
["","Výkon","P návrh","kW","2.50","3.40"]
["","Trieda energetickej účinnosti","","","A++","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Trieda energetickej účinnosti","","","A+","A+"]
["","Ročná spotreba energie","","kWh/rok","762","1,058"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","273","446"]
["","EER","","","4.57","3.81"]
["","COP","","","3.90","3.50"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","B"]
["Vykurovací výkon","Men.","","kW","3.20","4.20"]
["Poznámky","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Vonkajšia jednotka","","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Chladiaci výkon","Men.","","kW","","","5.00","5.70"]
["Vykurovací výkon","Men.","","kW","","","5.80","7.00"]
["Nominálna účinnosť","EER","","","","","3.24","3.05"]
["","COP","","","","","3.49","3.41"]
["","Ročná spotreba energie","","kWh","","","771","934"]
["","Smernica o energetickom označovaní","Chladenie","","","","A","B"]
["","","Vykurovanie","","","","B","B"]
["Chladenie","Trieda energetickej účinnosti","","","","","A+","A+"]
["","Výkon","P návrh","kW","","","5.00","5.70"]
["","SEER","","","","","5.98","5.76"]
["","Ročná spotreba energie","","kWh/rok","","","292","347"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","","A","A+"]
["","Výkon","P návrh","kW","","","3.84","3.96"]
["","SCOP/A","","","","","3.90","4.04"]
["","Pdh Vykurovací výkon pri -10°","","kW","","","3.51","3.66"]
["","Ročná spotreba energie","","kWh/rok","","","1377","1372"]