{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Chladiaci výkon","Men.","","kW","5.00","5.70"]
["Chladenie","Ročná spotreba energie","","kWh/a","","347"]
["","Výkon","P návrh","kW","","5.70"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","3.96"]
["","Ročná spotreba energie","","kWh/a","","1,372"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","771","934"]
["","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Smernica o energetickom označovaní","Chladenie","","A","B"]
["","","Vykurovanie","","B","B"]
["Vykurovací výkon","Men.","","kW","5.80","7.00"]
["Poznámky","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(3) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Chladenie","Trieda energetickej účinnosti","","","","A+"]
["","SEER","","","","5.76"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","A+"]
["","SCOP/A","","","","4.04"]