{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / RZASG71M2V1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7V1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7V1B"]
["Chladiaci výkon","Men.","","kW","6.80 (1)"]
["Chladenie","SEER","","","6.12"]
["","Ročná spotreba energie","","kWh/a","389"]
["","Výkon","P návrh","kW","6.80"]
["","Trieda energetickej účinnosti","","","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","4.50"]
["","SCOP/A","","","3.84"]
["","Trieda energetickej účinnosti","","","A"]
["","Ročná spotreba energie","","kWh/a","1,641"]
["Vykurovací výkon","Men.","","kW","7.50 (2)"]
["Poznámky","","","","(1) - Chladenie: T2: vnút. tepl. 26,6°CDB, 19,4°CWB, vonk. tepl. 48°CDB [Btu/h/W]","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Outdoor unit","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Chladiaci výkon","Men.","","kW","","9.50","9.50"]
["Vykurovací výkon","Men.","","kW","","10.8","10.8"]
["Chladenie","Trieda energetickej účinnosti","","","","A++","A"]
["","Výkon","P návrh","kW","","9.50","9.50"]
["","SEER","","","","6.24","5.49"]
["","Ročná spotreba energie","","kWh/a","","533","606"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","A","A"]
["","Výkon","P návrh","kW","","6.00","6.00"]
["","SCOP/A","","","","3.82","3.90"]
["","Ročná spotreba energie","","kWh/a","","2199","2154"]