{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZQG100L8Y1B","FFA50A2VEB / FFA50A2VEB / RZQG100L8Y1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZQG125L8Y1B","FFA50A2VEB / FFA50A2VEB / FFA50A2VEB / RZQG125L8Y1B","FFA60A2VEB / FFA60A2VEB / RZQG125L8Y1B","FFA50A2VEB / FFA50A2VEB / RZQG71L8Y1B","FFA35A2VEB / FFA35A2VEB / RZQG71L8Y1B"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Chladenie priestoru","SEER","","","","","","","","5.10","5.10"]
["","Ročná spotreba energie","","kWh/a","","","","","","467","467"]
["","Výkon","P návrh","kW","","","","","","6.80","6.80"]
["","Trieda energetickej účinnosti","","","","","","","","A","A"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","","","","","6.00","6.00"]
["","SCOP/A","","","","","","","","3.80","3.80"]
["","Trieda energetickej účinnosti","","","","","","","","A","A"]
["","Ročná spotreba energie","","kWh/a","","","","","","2,211","2,211"]
["Poznámky","","","","","","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","","","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]
["","","","","","","","","","","(3) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]