{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Opláštenie","Materiál","","","","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","260","260","260","260"]
["","","","Šírka","mm","575","575","575","575"]
["","","","Hĺbka","mm","575","575","575","575"]
["Hmotnosť","Jednotka","","","kg","16.0","16.0","17.5","17.5"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","9.0","10.0","12.0","14.5"]
["","","","Stredný","m³/min","8.0","8.5","10.0","12.5"]
["","","","Nízka","m³/min","6.5","6.5","7.5","9.5"]
["","","Kúrenie","Vysoké","m³/min","9.0","10.0","12.0","14.5"]
["","","Vykurovanie","Stredný","m³/min","8.0","8.5","10.0","12.5"]
["","","Kúrenie","Nízka","m³/min","6.5","6.5","7.5","9.5"]
["Akustický výkon","Chladenie","","","dBA","48","51","56","60"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","31.0","34.0","39.0","43.0"]
["","","","Stredný","dBA","28.5","30.5","34.0","40.0"]
["","","","Nízka","dBA","25.0","25.0","27.0","32.0"]
["","Kúrenie","","Vysoké","dBA","31.0","34.0","39.0","43.0"]
["","Vykurovanie","","Stredný","dBA","28.5","30.5","34.0","40.0"]
["","Kúrenie","","Nízka","dBA","25.0","25.0","27.0","32.0"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35","6.35","6.35"]
["","Plyn","","OD","mm","9.52","9.52","12.70","12.70"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Dekoračný panel","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Farba","","","","Biela (N9,5)","Biela (N9,5)","Biela (N9,5)","Biela (N9,5)"]
["","Vonkajšie rozmery","","Výška","mm","46","46","46","46"]
["","","","Šírka","mm","620","620","620","620"]
["","","","Hĺbka","mm","620","620","620","620"]
["","Hmotnosť","","","kg","2.8","2.8","2.8","2.8"]
["Dekoračný panel 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Farba","","","","Strieborný","Strieborný","Strieborný","Strieborný"]
["","Vonkajšie rozmery","","Výška","mm","46","46","46","46"]
["","","","Šírka","mm","620","620","620","620"]
["","","","Hĺbka","mm","620","620","620","620"]
["","Hmotnosť","","","kg","2.8","2.8","2.8","2.8"]
["Dekoračný panel 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Farba","","","","Biela (RAL9010)","Biela (RAL9010)","Biela (RAL9010)","Biela (RAL9010)"]
["","Vonkajšie rozmery","","Výška","mm","55","55","55","55"]
["","","","Šírka","mm","700","700","700","700"]
["","","","Hĺbka","mm","700","700","700","700"]
["","Hmotnosť","","","kg","2.7","2.7","2.7","2.7"]
["Dekoračný panel 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Farba","","","","Biela (RAL9010)","Biela (RAL9010)","Biela (RAL9010)","Biela (RAL9010)"]
["","Vonkajšie rozmery","","Výška","mm","55","55","55","55"]
["","","","Šírka","mm","700","700","700","700"]
["","","","Hĺbka","mm","700","700","700","700"]
["","Hmotnosť","","","kg","2.7","2.7","2.7","2.7"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","BRC7EB530 (štandardný panel), BRC7F530W (biely panel), BRC7F530S (sivý panel)","BRC7EB530 (štandardný panel), BRC7F530W (biely panel), BRC7F530S (sivý panel)","BRC7EB530 (štandardný panel), BRC7F530W (biely panel), BRC7F530S (sivý panel)","BRC7EB530 (štandardný panel), BRC7F530W (biely panel), BRC7F530S (sivý panel)"]
["","Káblový diaľkový ovládač","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Štandardné príslušenstvo","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Napájanie","Fáza","","","","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240"]