{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50A5V1B","FFA60A2VEB9 / RXM60A5V1B"]
["Chladiaci výkon","Men.","","kW","5.00","5.7"]
["Vykurovací výkon","Men.","","kW","5.80","7"]
["Nominálna účinnosť","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Ročná spotreba energie","","kWh","772","931"]
["","Smernica o energetickom označovaní","Chladenie","","A","B"]
["","","Vykurovanie","","B","B"]
["Chladenie","Trieda energetickej účinnosti","","","A+","A+"]
["","Výkon","P návrh","kW","5.00","5.7"]
["","SEER","","","5.98","5.76"]
["","Ročná spotreba energie","","kWh/a","293","346"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A","A+"]
["","Výkon","P návrh","kW","3.84","3.96"]
["","SCOP/A","","","3.90","4.04"]
["","Pdh Vykurovací výkon pri -10°","","kW","3.40","3.5"]
["","Ročná spotreba energie","","kWh/a","1378","1373"]
["Poznámky","","","","","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["","","","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","(4) - Elektrické údaje nájdete v samostatných nákresoch"]