{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":26,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9)"]
[]
[]
[]
[]
["","","","","","FHA35AVEB99","FHA35AVEB98","FHA35AVEB9","FHA50AVEB9","FHA50AVEB99","FHA50AVEB98","FHA60AVEB9","FHA60AVEB99","FHA60AVEB98","FHA71AVEB99","FHA71AVEB9","FHA71AVEB98","FHA100AVEB","FHA100AVEB8","FHA100AVEB9","FHA125AVEB","FHA125AVEB8","FHA125AVEB9","FHA140AVEB","FHA140AVEB8"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","","","","","","","","","","","","","","","","","14.00","","","15.40"]
["Opláštenie","Farba","","","","Biela","Biela","Biela","Biela","Biela","Biela","Biela","","Biela","","","Biela","","Biela","","","Biela","","","Biela"]
["","Materiál","","","","Živica, oceľový plech","Živica, oceľový plech","Živica, oceľový plech","Živica, oceľový plech","Živica, oceľový plech","Živica, oceľový plech","Živica, oceľový plech","","Živica, oceľový plech","","","Živica, oceľový plech","","Živica, oceľový plech","","","Živica, oceľový plech","","","Živica, oceľový plech"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","235","235","235","235","235","235","235","","235","","","235","","235","","","235","","","235"]
["","","","Šírka","mm","960","960","960","960","960","960","1270","","1270","","","1270","","1590","","","1590","","","1590"]
["","","","Hĺbka","mm","690","690","690","690","690","690","690","","690","","","690","","690","","","690","","","690"]
["Hmotnosť","Jednotka","","","kg","24.0","26","24","25","25.0","27","31","31.0","32","32.0","32","34","38.0","41","38.0","38.0","41","38.0","38.0","41","38.0"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","14.0","14.0","14.0","15.0","15.0","15.0","19.5","","19.5","","","20.5","","28.0","","","31.0","","","34.0"]
["","","","Stredný","m³/min","11.5","11.5","11.5","12.0","12.0","12.0","15.0","","15.0","","","17.0","","24.0","","","27.0","","","29.0"]
["","","","Nízka","m³/min","10.0","10.0","10.0","10.0","10.0","10.0","11.5","","11.5","","","14.0","","20.0","","","23.0","","","24.0"]
["","","Kúrenie","Vysoké","m³/min","14.0","14.0","14.0","15.0","15.0","15.0","19.5","","19.5","","","20.5","","28.0","","","31.0","","","34.0"]
["","","Vykurovanie","Stredný","m³/min","11.5","11.5","11.5","12.0","12.0","12.0","15.0","","15.0","","","17.0","","24.0","","","27.0","","","29.0"]
["","","Kúrenie","Nízka","m³/min","10.0","10.0","10.0","10.0","10.0","10.0","11.5","","11.5","","","14.0","","20.0","","","23.0","","","24.0"]
["Akustický výkon","Chladenie","","","dBA","53","53.0","53.0","54.0","54","54.0","54.0","","54.0","","","55.0","","60.0","","","62.0","","","64.0"]
["","Vykurovanie","","","dBA","","53.0","","","","54.0","","","54.0","","","55.0","","60.0","","","62.0","","","64.0"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","36","36.0","36.0","37.0","37","37.0","37.0","","37.0","","","38.0","","42.0","","","44.0","","","46.0"]
["","","","Stredný","dBA","34","34.0","34.0","35.0","35","35.0","35.0","","35.0","","","36.0","","38.0","","","41.0","","","42.0"]
["","","","Nízka","dBA","31","31.0","31.0","32.0","32","32.0","33.0","","33.0","","","34.0","","34.0","","","37.0","","","38.0"]
["","Kúrenie","","Vysoké","dBA","36","36.0","36.0","37.0","37","37.0","37.0","","37.0","","","38.0","","42.0","","","44.0","","","46.0"]
["","Vykurovanie","","Stredný","dBA","31","31.0","31.0","32.0","32","32.0","33.0","","33.0","","","34.0","","34.0","","","37.0","","","38.0"]
["","Kúrenie","","Men.","dBA","34","34.0","34.0","35.0","35","35.0","35.0","","35.0","","","36.0","","38.0","","","41.0","","","42.0"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.40","6.35","6.35","6.35","6.40","6.35","6.35","","6.35","","","9.52","","9.52","","","9.52","","","9.52"]
["","Plyn","","OD","mm","9.50","9.50","9.5","12.7","12.7","12.70","12.7","","12.70","","","15.90","","15.90","","","15.90","","","15.90"]
["","Odvod kondenzátu","","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20","","VP20","","","VP20","","VP20","","","VP20","","","VP20"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","BRC7GA53, BRC7GA56","BRC7F530W (biely panel), BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7F530W (biely panel), BRC7GA56","BRC7GA53, BRC7GA56","","BRC7F530W (biely panel), BRC7GA56","","","BRC7F530W (biely panel), BRC7GA56","","BRC7F530W (biely panel), BRC7GA56","","","BRC7F530W (biely panel), BRC7GA56","","","BRC7F530W (biely panel), BRC7GA56"]
["","Káblový diaľkový ovládač","","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K","","","BRC1D528, BRC1H51(9)W/S/K7, BRC1H52W/S/K, BRC1H81W7, BRC1H81S7, BRC1E53A/B/C7, BRC1H82W/S/K"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~","1~","","1~","","","1~","","1~","","","1~","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50/60","50","50","50","50/60","50","","50/60","","","50/60","","50/60","","","50/60","","","50/60"]
["","Napätie","","","V","220-240","220-240/220","220-240","220-240","220-240","220-240/220","220-240","","220-240/220","","","220-240/220","","220-240/220","","","220-240/220","","","220-240/220"]
["Štandardné príslušenstvo","Thermal insulation tube","","","","2","2","2","2","2","2","2","","2","","","2","","2","","","2","","","2"]
["","Resin bushing","","","","1","1","1","1","1","1","1","","1","","","1","","1","","","1","","","1"]
["","Wiring fixture","","","","2","2","2","2","2","2","2","","2","","","2","","2","","","2","","","2"]
["","Hose band","","","","1","1","1","1","1","1","1","","1","","","1","","1","","","1","","","1"]
["","Wire clamp material","","","","7","7","7","7","7","7","7","","7","","","7","","7","","","7","","","7"]
["","Drain hose","","","","1","1","1","1","1","1","1","","1","","","1","","1","","","1","","","1"]
["","Screws","","","","2","2","2","2","2","2","2","","2","","","2","","2","","","2","","","2"]
["","Sealing pad (large)","","","","1","","1","1","1","","1"]
["","Sealing pad (small)","","","","1","","1","1","1","","1"]
["","Washer","","","","8","8","8","8","8","8","8","","8","","","8","","8","","","8","","","8"]
["Poznámky","","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["Štandardné príslušenstvo","General safety precautions","","","","","1","","","","1","","","1","","","1","","1","","","1","","","1"]
["","Installation and operation manual","","","","","1","","","","1","","","1","","","1","","1","","","1","","","1"]
["","Paper pattern for installation","","","","","1","","","","1","","","1","","","1","","1","","","1","","","1"]
["","Sealing material","","","","","6","","","","6","","","6","","","6","","6","","","6","","","6"]