{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Chladiaci výkon","Men.","","kW","3.40"]
["Chladenie priestoru","SEER","","","6.24"]
["","Ročná spotreba energie","","kWh/a","191"]
["","Výkon","P návrh","kW","3.40"]
["","Trieda energetickej účinnosti","","","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Trieda energetickej účinnosti","","","A+"]
["","Ročná spotreba energie","","kWh/a","979"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Smernica o energetickom označovaní","Chladenie","","A"]
["","","Vykurovanie","","A"]
["Vykurovací výkon","Men.","","kW","4.00"]
["Poznámky","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Vonkajšia jednotka","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Chladiaci výkon","Men.","","kW","","5.00","5.70"]
["Vykurovací výkon","Men.","","kW","","6.00","7.20"]
["Nominálna účinnosť","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Ročná spotreba energie","","kWh","","780","867"]
["","Smernica o energetickom označovaní","Chladenie","","","B","A"]
["","","Vykurovanie","","","C","C"]
["Chladenie","Trieda energetickej účinnosti","","","","A+","A+"]
["","Výkon","P návrh","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Ročná spotreba energie","","kWh/a","","295","328"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","A","A"]
["","Výkon","P návrh","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Vykurovací výkon pri -10°","","kW","","3.85","4.08"]
["","Ročná spotreba energie","","kWh/a","","1578","1704"]