{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":16,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Chladenie","SEER","","","6.95","5.10","5.10","6.86","5.10","6.11","5.10","5.10","5.10","5.10","6.01"]
["","Ročná spotreba energie","","kWh/rok","343","467","467","347","467","545","652","652","652","824","699"]
["","Výkon","P návrh","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Trieda energetickej účinnosti","","","A++","B","B","A++","B","A++","B","B","B","B","A+"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","7.60","6.00","6.00","7.60","6.00","11.30","11.30","11.30","11.30","12.71","14.13"]
["","SCOP/A","","","4.32","3.80","3.80","4.32","3.80","4.61","3.80","3.80","3.80","3.80","4.23"]
["","Trieda energetickej účinnosti","","","A+","A","A","A+","A","A++","A","A","A","A","A+"]
["","Ročná spotreba energie","","kWh/rok","2,463","2,211","2,211","2,463","2,211","3,432","4,164","4,164","4,164","4,683","4,677"]
["Chladiaci výkon","Men.","","kW","","","","6.8","","","","","","","","13.4"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","","","890","","","","","","","","2,025"]
["","EER","","","","","","3.82","","","","","","","","3.31"]
["","COP","","","","","","4.13","","","","","","","","3.63"]
["","Smernica o energetickom označovaní","Chladenie","","","","","A","","","","","","","","A"]
["","","Vykurovanie","","","","","A","","","","","","","","A"]
["Vykurovací výkon","Men.","","kW","","","","7.5","","","","","","","","15.5"]
["Poznámky","","","","","","","(1) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES","","","","","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","","","","(2) - Hodnoty SEER a SCOP sú podľa normy EN 14825","","","","","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]