{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","46"]
["","","Tichá prevádzka","dBA","30"]
["","","Nízka","dBA","33"]
["","Chladenie","Tichá prevádzka","dBA","29"]
["","","Nízka","dBA","32"]
["","","Vysoké","dBA","38"]
["","","Men.","dBA","36"]
["","Chladenie","Men.","dBA","35"]
["Štandardné príslušenstvo","Návod na montáž","","","1"]
["","Návod na prevádzku","","","1"]
["","Infračervené diaľkové ovládanie","","","1"]
["","Batérie so suchými článkami typu AAA","","","2"]
["","Držiak diaľkového ovládača","","","1"]
["","Montážna platnička","","","1"]
["","Tepelná izolačná trubica (potrubie s chladivom)","","","8"]
["","Filter na čistenia vzduchu","","","1"]
["","Fotokatalytický dezodoračný filter","","","1"]
["","Bočný kryt","","","2"]
["","Spojovacie pásmo","","","4"]
["Control systems","Infrared remote control","","","ARC433B67"]
["Pripojenia potrubí","Kvapalný","OD","mm","6.35"]
["","Plyn","OD","mm","9.5"]
["","Vypúšťanie","","","18"]
["Akustický výkon","Chladenie","","dBA","53"]
["","Vykurovanie","","dBA","59"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","1,050"]
["","","Hĺbka","mm","200"]
["","","Výška","mm","490"]
["Casing","Farba","","","Biela mandľa"]
["Hmotnosť","Jednotka","","kg","16"]
["Power supply","Fáza","","","1~"]
["","Frekvencia","","Hz","50"]
["","Názov","","","VM"]
["","Napätie","","V","220-240"]
["Poznámky","","","","(1) - 220 V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť."]