{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","42","44","46","39","40","41"]
["","","Tichá prevádzka","dBA","30","32","34","25","25","26"]
["","","Nízka","dBA","33","35","37","28","28","29"]
["","Chladenie","Tichá prevádzka","dBA","31","33","34","22","22","23"]
["","","Nízka","dBA","34","36","37","25","26","27"]
["","","Vysoké","dBA","43","45","46","39","40","41"]
["","","Men.","dBA","38","40","42","34","34","35"]
["","Chladenie","Men.","dBA","39","41","42","33","33","34"]
["Štandardné príslušenstvo","Návod na montáž","","","1","1","1","1","1","1"]
["","Návod na prevádzku","","","1","1","1","1","1","1"]
["","Bezdrôtové diaľkové ovládanie","","","1","1","1","1","1","1"]
["","Batérie","","","2","2","2","2","2","2"]
["","Držiak diaľkového ovládača","","","1","1","1","1","1","1"]
["","Montážna platnička","","","1","1","1","1","1","1"]
["","Upevňovacia skrutka pre vnútornú jednotku","","","","","","2","2","2"]
["","Titánovo apatitový fotokatalytický filter na čistenie vzduchu","","","2","2","2","2","2","2"]
["Control systems","Infra. diaľkové ovládanie","","","ARC433B70","ARC433B70","ARC433B70"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Vypúšťanie","","","18","18","18","18","18","18"]
["Vstup napájania","Chladenie","Men.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Kúrenie","Men.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Úroveň akustického výkonu","Chladenie","","dBA","59","60","63","55","56","57"]
["","Vykurovanie","","dBA","58","59","62","55","56","57"]
["Vonkajšie rozmery","Jednotka","Width","mm","1,050","1,050","1,050","770","770","770"]
["","","Hĺbka","mm","238","238","238","198","198","198"]
["","","Height","mm","290","290","290","283","283","283"]
["Opláštenie","Farba","","","Biela","Biela","Biela","Biela","Biela","Biela"]
["Hmotnosť","Unit","","kg","12","12","12","7","7","7"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50","50","50","50","50","50"]
["","Name","","","V1","V1","V1","V1","V1","V1"]
["","Napätie","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Štandardné príslušenstvo","Upevňovacie skrutky vnútornej jednotky","","","2","2"]
["Poznámky","","","","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu"]
["","","","","(2) - 220 V","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V","(4) - 240 V"]
["Štandardné príslušenstvo","Upevňovacie skrutky vnútornej jednotky (M4 x 12L)","","","","","2"]