{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.03","0.030","0.030"]
["","Kúrenie","","Men.","kW","0.04","0.040","0.040"]
["Opláštenie","Farba","","","","Biela","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","198","198","198"]
["","","","Šírka","mm","770","770","770"]
["","","","Hĺbka","mm","283","283","283"]
["Hmotnosť","Jednotka","","","kg","7","7.00","7.00"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","9.1","9.2","9.3"]
["","","","Stredný","m³/min","7.4","7.6","7.7"]
["","","","Nízka","m³/min","5.9","6.0","6.1"]
["","","","Tichá prevádzka","m³/min","4.7","4.8","4.9"]
["","","Kúrenie","Vysoké","m³/min","9.4","9.7","10.1"]
["","","Vykurovanie","Stredný","m³/min","7.8","8.0","8.4"]
["","","Kúrenie","Nízka","m³/min","6.3","6.3","6.7"]
["","","","Tichá prevádzka","m³/min","5.5","5.5","5.7"]
["Akustický výkon","Chladenie","","","dBA","55","55","58"]
["","Vykurovanie","","","dBA","55","55","58"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","39","40","41"]
["","","","Stredný","dBA","33","33","34"]
["","","","Nízka","dBA","25","26","27"]
["","","","Tichá prevádzka","dBA","22","22","23"]
["","Kúrenie","","Vysoké","dBA","39","40","41"]
["","Vykurovanie","","Stredný","dBA","34","34","35"]
["","Kúrenie","","Nízka","dBA","28","28","29"]
["","","","Tichá prevádzka","dBA","25","25","26"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35","6.35"]
["","Plyn","","OD","mm","9.5","9.50","9.50"]
["","Odvod kondenzátu","","","","18","18","18"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARC433A87","ARC433A87","ARC433A87"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Napájanie","Názov","","","","V1","V1","V1"]
["","Fáza","","","","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240"]