{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","39","40","41","","46"]
["","","","Stredný","dBA","32","33","33","","42"]
["","","","Tichá prevádzka","dBA","19","19","19","","24"]
["","","","Nízka","dBA","25","25","25","","33"]
["","Chladenie","","Stredný","dBA","32","33","33","","39"]
["","","","Tichá prevádzka","dBA","19","19","19","","24"]
["","","","Nízka","dBA","25","25","25","","31"]
["","","","Vysoké","dBA","39","40","41","","46"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","1","1","","1"]
["","Návod na prevádzku","","","","1","1","1","","1"]
["","Vzduchový filter","","","","2","2","2","","2"]
["","Infračervené diaľkové ovládanie","","","","1","1","1","","1"]
["","Montážna platnička diaľkového ovládača","","","","1","1","1","","1"]
["","Nádobka na skrutky","","","","1","1","1","","1"]
["","Kryt na skrutky","","","","1","1","1","","1"]
["","Batérie so suchými článkami typu AAA","","","","2","2","2","","2"]
["","Všeobecné bezpečnostné opatrenia","","","","1","1","1","","1"]
["Chladiace médium","GWP","","","","675.0","675.0","675.0","","675.0"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infra. diaľkové ovládanie","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Pripojenia potrubí","Kvapalina","","OD","mm","6.35","6.35","6.35","","6.35"]
["","Plyn","","OD","mm","9.50","9.50","9.50","","12.70"]
["","Vypúšťanie","","","","18","18","18","","18"]
["Vstup napájania","Chladenie","","Men.","kW","0.020","0.022","0.023","","0.030"]
["","Kúrenie","","Men.","kW","0.020","0.020","0.022","","0.039"]
["Akustický výkon","Chladenie","","","dBA","57","57","60","","60"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","798","798","798","","798"]
["","","","Hĺbka","mm","189","189","189","","189"]
["","","","Výška","mm","295","295","295","","295"]
["Opláštenie","Farba","","","","Biela","Biela","Biela","","Biela"]
["Hmotnosť","Jednotka","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Stredný","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Nízka","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Tichá prevádzka","m³/min","4.5","4.5","4.5","","5.7"]
["","","Chladenie","Nízka","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Stredný","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Vysoké","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Tichá prevádzka","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Fáza","","","","1~","1~","1~","","1~"]
["","Názov","","","","V1","V1","V1","","V1"]
["","Frekvencia","","","Hz","50","50","50","","50"]
["","Napätie","","","V","220-240","220-240","220-240","","220-240"]
["Vstup napájania","Chladenie","","Men.","kW","","","","0.028"]
["","Kúrenie","","Men.","kW","","","","0.036"]
["Opláštenie","Farba","","","","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","","295"]
["","","","Šírka","mm","","","","798"]
["","","","Hĺbka","mm","","","","189"]
["Hmotnosť","Jednotka","","","kg","","","","11.50"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","","","13.1"]
["","","","Stredný","m³/min","","","","9.8"]
["","","","Nízka","m³/min","","","","7.2"]
["","","","Tichá prevádzka","m³/min","","","","4.6"]
["","","Kúrenie","Vysoké","m³/min","","","","14.6"]
["","","Vykurovanie","Stredný","m³/min","","","","10.5"]
["","","Kúrenie","Nízka","m³/min","","","","7.7"]
["","","","Tichá prevádzka","m³/min","","","","5.2"]
["Akustický výkon","Chladenie","","","dBA","","","","60"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","","","45"]
["","","","Stredný","dBA","","","","37"]
["","","","Nízka","dBA","","","","29"]
["","","","Tichá prevádzka","dBA","","","","21"]
["","Kúrenie","","Vysoké","dBA","","","","45"]
["","Vykurovanie","","Stredný","dBA","","","","37"]
["","Kúrenie","","Nízka","dBA","","","","29"]
["","","","Tichá prevádzka","dBA","","","","21"]
["Chladivo","GWP","","","","","","","675.0"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","","","6.35"]
["","Plyn","","OD","mm","","","","12.70"]
["","Odvod kondenzátu","","","","","","","18"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","","","","ARC466A58"]
["","Káblový diaľkový ovládač","","","","","","","BRC073"]
["Štandardné príslušenstvo","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Vzduchový filter","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Napájanie","Názov","","","","","","","V1"]
["","Fáza","","","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","","50"]
["","Napätie","","","V","","","","220-240"]