{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B / 3MXF-A9"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B / FTXF20B5V1B / FTXF20B5V1B / 3MXF52A2V1B9","FTXF20B5V1B / FTXF25B5V1B / FTXF25B5V1B / 3MXF68A2V1B9"]
["Chladiaci výkon","Min.","","kW","1.80","2.00"]
["","Max.","","kW","7.00","7.20"]
["","Men.","","kW","5.20","6.80"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","634","977"]
["","EER","","","4.10","3.48"]
["","COP","","","3.93","3.82"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","A"]
["Vykurovací výkon","Men.","","kW","6.80","8.60"]
["","Min.","","kW","1.30","2.20"]
["","Max.","","kW","8.00","10.50"]
["Chladenie priestoru","SEER","","","","6.61"]
["","Ročná spotreba energie","","kWh/a","","360"]
["","Výkon","P návrh","kW","","6.80"]
["","Trieda energetickej účinnosti","","","","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","5.30"]
["","SCOP/A","","","","4.03"]
["","Trieda energetickej účinnosti","","","","A+"]
["","Ročná spotreba energie","","kWh/a","","1,843"]