{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B / RXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B / RXF20B5V1B","FTXF25B5V1B / RXF25B5V1B"]
["Vonkajšia jednotka","","","","RXF20B5V1B","RXF25B5V1B"]
["Chladiaci výkon","Min.","","kW","1.3","1.3"]
["","Men.","","kW","2.00","2.50"]
["","Max.","","kW","2.6","3.0"]
["Vykurovací výkon","Min.","","kW","1.30","1.30"]
["","Men.","","kW","2.50","2.80"]
["","Max.","","kW","3.50","4.00"]
["Nominálna účinnosť","EER","","","3.94","3.30"]
["","COP","","","4.19","4.01"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","A"]
["Chladenie","Trieda energetickej účinnosti","","","A++","A++"]
["","Výkon","P návrh","kW","2.00","2.50"]
["","SEER","","","6.15","6.22"]
["","Ročná spotreba energie","","kWh/a","114","141"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A+","A+"]
["","Výkon","P návrh","kW","2.20","2.40"]
["","SCOP/A","","","4.10","4.06"]
["","Pdh Vykurovací výkon pri -10°","","kW","1.99","2.10"]
["","Ročná spotreba energie","","kWh/a","751","827"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D","A+++ ~ D"]
["Poznámky","","","","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","(3) - Elektrické údaje nájdete v samostatných nákresoch"]