{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Chladiaci výkon","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.0","4.6"]
["","Men.","","kW","2.5 (2)","3.5 (2)"]
["Pripojenia potrubia","Kvapalina","OD","mm","6.35","6.35"]
["","Plyn","OD","mm","9.5","9.5"]
["","Vypúšťanie","OD","mm","18","18"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","340","490"]
["","EER","","","3.68 (1)","3.57 (1)"]
["","COP","","","4.31 (1)","3.89 (1)"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","A"]
["Vykurovací výkon","Men.","","kW","4.4 (2)","5.1 (2)"]
["","Min.","","kW","1.0 (6)","1.0 (6)"]
["","Max.","","kW","6.1, 3.6 (7)","6.7, 4.2 (7)"]
["Poznámky","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]
["","","","","(3) - 220 V","(3) - 220 V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240 V","(5) - 240 V"]
["","","","","(6) - Pre nominálny minimálny vykurovací výkon je ventilátor vnútornej jednotky nastavený na SL","(6) - Pre nominálny minimálny vykurovací výkon je ventilátor vnútornej jednotky nastavený na SL"]
["","","","","(7) - Maximálny vykurovací výkon pri vonkajšej teplote -15°C","(7) - Maximálny vykurovací výkon pri vonkajšej teplote -15°C"]