{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / RXJ20M2V1B","FTXJ20MV1BW / RXJ20M3V1B","FTXJ20MV1BW / RXJ20M5V1B","FTXJ25MV1BW / RXJ25M2V1B","FTXJ25MV1BW / RXJ25M5V1B","FTXJ25MV1BW / RXJ25M3V1B","FTXJ35MV1BW / RXJ35M5V1B","FTXJ35MV1BW / RXJ35M2V1B","FTXJ35MV1BW / RXJ35M3V1B","FTXJ50MV1BW / RXJ50MV1B"]
["Chladiaci výkon","Min.","","kW","","1.30","","","","0.90"]
["","Max.","","kW","","2.80","","","","3.30"]
["","Men.","","kW","2.3","2.30","2.30","2.4","2.40","2.40","3.50","3.5","","4.80"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","248","248","248","254","254","254","428","428","","716"]
["","EER","","","4.64","4.64","4.64","4.73","4.73","4.73","4.09","4.09","","3.35"]
["","COP","","","5.00","5.00","5.00","4.57","4.57","4.57","4.04","4.04","","3.65"]
["","Smernica o energetickom označovaní","Chladenie","","A","A","A","A","A","A","A","A","","A"]
["","","Vykurovanie","","A","A","A","A","A","A","A","A","","A"]
["Vykurovací výkon","Men.","","kW","2.5","2.50","2.5","3.2","3.2","3.20","4.0","4","","5.80"]
["","Min.","","kW","","1.30","","","","0.90"]
["","Max.","","kW","","4.30","","","","4.70"]
["Poznámky","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","(2) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]
["","","","","","(1) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(1) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","","(1) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(1) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(1) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]
["Chladiaci výkon","Min.","","kW","","","","","","","","","0.90"]
["","Men.","","kW","","","","","","","","","3.50"]
["","Max.","","kW","","","","","","","","","4.10"]
["Vykurovací výkon","Min.","","kW","","","","","","","","","0.90"]
["","Men.","","kW","","","","","","","","","4.00"]
["","Max.","","kW","","","","","","","","","5.10"]
["Nominálna účinnosť","EER","","","","","","","","","","","4.09"]
["","COP","","","","","","","","","","","4.04"]
["","Ročná spotreba energie","","kWh","","","","","","","","","428"]
["","Smernica o energetickom označovaní","Chladenie","","","","","","","","","","A"]
["","","Vykurovanie","","","","","","","","","","A"]
["Chladenie","Trieda energetickej účinnosti","","","","","","","","","","","A++"]
["","Výkon","P návrh","kW","","","","","","","","","3.50"]
["","SEER","","","","","","","","","","","7.19"]
["","Ročná spotreba energie","","kWh/rok","","","","","","","","","170"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","","","","","","","","A++"]
["","Výkon","P návrh","kW","","","","","","","","","3.00"]
["","SCOP/A","","","","","","","","","","","4.60"]
["","Pdh Vykurovací výkon pri -10°","","kW","","","","","","","","","2.61"]
["","Ročná spotreba energie","","kWh/rok","","","","","","","","","913"]