{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV / RXL-M"]
[]
[]
[]
[]
["","","","","FTXL25J2V1B / RXL25M2V1B","FTXL35J2V1B / RXL35M2V1B"]
["Chladiaci výkon","Min.","","kW","1.2","1.3"]
["","Max.","","kW","3.4","3.8"]
["Pripojenia potrubia","Kvapalina","OD","mm","6.35","6.35"]
["","Plyn","OD","mm","9.5","9.5"]
["","Drain","OD","mm","18","18"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","400.5","570"]
["","EER","","","3.12","3.07"]
["","COP","","","4.43","4.21"]
["","Smernica o energetickom označovaní","Chladenie","","B","B"]
["","","Vykurovanie","","A","A"]
["Vykurovací výkon","Min.","","kW","1.1","1.2"]
["","Max.","","kW","5.5","6.0"]
["Poznámky","","","","(1) - Pre nominálny minimálny vykurovací výkon je ventilátor vnútornej jednotky nastavený na SL","(1) - Pre nominálny minimálny vykurovací výkon je ventilátor vnútornej jednotky nastavený na SL"]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]
["","","","","(5) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","(5) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","(6) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž","(6) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]