{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","47","47"]
["","","Tichá prevádzka","dBA","19","19"]
["","","Nízka","dBA","23","23"]
["","Chladenie","Tichá prevádzka","dBA","21","21"]
["","","Nízka","dBA","33","33"]
["","","Vysoké","dBA","45","45"]
["","","Men.","dBA","37","36"]
["","Chladenie","Men.","dBA","39","39"]
["Štandardné príslušenstvo","Návod na montáž","","","1","1"]
["","Návod na prevádzku","","","1","1"]
["","Infračervené diaľkové ovládanie","","","1","1"]
["","Batérie","","","2","2"]
["","Držiak diaľkového ovládača","","","1","1"]
["","Montážna platnička","","","1","1"]
["","Titánovo apatitový fotokatalytický filter na čistenie vzduchu","","","2","2"]
["","Upevňovacie skrutky vnútornej jednotky","","","2","2"]
["Riadiace systémy","Infrared remote control","","","ARC466A9","ARC466A9"]
["Pripojenia potrubí","Kvapalina","OD","mm","6.35","6.35"]
["","Plyn","OD","mm","9.5","9.5"]
["","Vypúšťanie","","","18","18"]
["Príkon","Chladenie","Men.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Kúrenie","Men.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Chladenie","","dBA","59","59"]
["","Vykurovanie","","dBA","62","62"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","900","900"]
["","","Hĺbka","mm","215","215"]
["","","Výška","mm","298","298"]
["Opláštenie","Farba","","","Biela","Biela"]
["Hmotnosť","Jednotka","","kg","12","12"]
["Power supply","Fáza","","","1~","1~"]
["","Frekvencia","","Hz","50","50"]
["","Názov","","","V1","V1"]
["","Napätie","","V","220-240","220-240"]
["Poznámky","","","","(1) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť.","(1) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]