{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Chladiaci výkon","Men.","","kW","4.00"]
["Vykurovací výkon","Men.","","kW","4.20"]
["Nominálna účinnosť","EER","","","3.71"]
["","COP","","","3.75"]
["","Ročná spotreba energie","","kWh","539"]
["","Smernica o energetickom označovaní","Chladenie","","A"]
["","","Vykurovanie","","A"]
["Chladenie","Trieda energetickej účinnosti","","","A++"]
["","Výkon","P návrh","kW","4.00"]
["","SEER","","","7.74"]
["","Ročná spotreba energie","","kWh/a","181"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A+"]
["","Výkon","P návrh","kW","3.20"]
["","SCOP/A","","","4.30"]
["","Pdh Vykurovací výkon pri -10°","","kW","2.46"]
["","Ročná spotreba energie","","kWh/a","1041"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D"]
["Poznámky","","","","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["","","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(4) - Elektrické údaje nájdete v samostatných nákresoch","(4) - Elektrické údaje nájdete v samostatných nákresoch"]
["Chladiaci výkon","Men.","","kW","","4.00"]
["Vykurovací výkon","Men.","","kW","","5.20"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","554"]
["","COP","","","","3.68"]
["","EER","","","","3.61"]
["","Smernica o energetickom označovaní","Chladenie","","","A"]
["","","Vykurovanie","","","A"]