{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","38","39","42","42","44","","46"]
["","","","Tichá prevádzka","dBA","25","25","26","30","31","","34"]
["","","","Nízka","dBA","28","28","29","33","34","","37"]
["","Chladenie","","Tichá prevádzka","dBA","22","22","23","30","31","","34"]
["","","","Nízka","dBA","25","25","26","33","34","","37"]
["","","","Vysoké","dBA","38","38","42","42","43","","46"]
["","","","Men.","dBA","33","34","36","38","39","","42"]
["","Chladenie","","Men.","dBA","32","32","34","38","39","","42"]
["Štandardné príslušenstvo","Titánovo apatitový fotokatalytický filter na čistenie vzduchu","","","","2","2","2","2","2"]
["","Návod na prevádzku","","","","1","1","1","1","1","","1"]
["","Návod na montáž","","","","1","1","1","1","1","","1"]
["","Bezdrôtové diaľkové ovládanie","","","","1","1","1","1","1","","1"]
["","Batérie","","","","2","2","2","2","2","","2"]
["","Držiak diaľkového ovládača","","","","1","1","1","1","1","","1"]
["","Upevňovacie skrutky vnútornej jednotky","","","","2","2","2","2","2","","2"]
["","Montážna platnička","","","","1","1","1","1","1","","1"]
["Control systems","Infra. diaľkové ovládanie","","","","","","","","","","ARC452A3"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Plyn","","OD","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Vypúšťanie","","","","18","18","18","18","18","","18"]
["Vstup napájania","Chladenie","","Men.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Kúrenie","","Men.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Úroveň akustického výkonu","Chladenie","","","dBA","54","54","58","58","59","","63"]
["","Vykurovanie","","","dBA","54","55","58","58","60","","62"]
["Vonkajšie rozmery","Jednotka","","Width","mm","800","800","800","800","800","","1,050"]
["","","","Hĺbka","mm","215","215","215","215","215","","250"]
["","","","Výška","mm","295","295","295","295","295","","290"]
["Casing","Farba","","","","Biela","Biela","Biela","Biela","Biela","","Biela"]
["Hmotnosť","Jednotka","","","kg","9","9","10","10","10","","12"]
["Power supply","Fáza","","","","1~","1~","1~","1~","1~","","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","","50"]
["","Name","","","","V1","V1","V1","V1","V1","","V1"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V"]
["Ventilátor","Prietok vzduchu","Chladenie","Men.","m³/min","","","","","","16.0"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","","","","","","41"]
["Ventilátor","Prietok vzduchu","Kúrenie","Men.","m³/min","","","","","","14.9"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","","","","","","40"]
["Vstup napájania","Chladenie","","Men.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Kúrenie","","Men.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Opláštenie","Farba","","","","","","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","","","","290"]
["","","","Šírka","mm","","","","","","1050"]
["","","","Hĺbka","mm","","","","","","250"]
["Hmotnosť","Jednotka","","","kg","","","","","","12"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","","","","","16.0"]
["","","","Nízka","m³/min","","","","","","11.3"]
["","","","Tichá prevádzka","m³/min","","","","","","10.1"]
["","","Kúrenie","Vysoké","m³/min","","","","","","17.2"]
["","","","Nízka","m³/min","","","","","","12.6"]
["","","","Tichá prevádzka","m³/min","","","","","","11.3"]
["Akustický výkon","Chladenie","","","dBA","","","","","","60"]
["","Vykurovanie","","","dBA","","","","","","59"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","","","","","45"]
["","","","Nízka","dBA","","","","","","36"]
["","","","Tichá prevádzka","dBA","","","","","","33"]
["","Kúrenie","","Vysoké","dBA","","","","","","44"]
["","","","Nízka","dBA","","","","","","35"]
["","","","Tichá prevádzka","dBA","","","","","","32"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","","","","","6.35"]
["","Plyn","","OD","mm","","","","","","12.7"]
["","Odvod kondenzátu","","","","","","","","","18"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","","","","","","ARC452A3"]
["Štandardné príslušenstvo","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Napájanie","Názov","","","","","","","","","V1"]
["","Fáza","","","","","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","","","","50"]
["","Napätie","","","V","","","","","","220-240"]
["Štandardné príslušenstvo","Titánovo apatitový fotokatalytický filter na čistenie vzduchu bez rámu","","","","","","","","","","2"]
["Poznámky","","","","","","","","","","","(4) - 240 V"]