{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","40","","","","","","45"]
["","","","Tichá prevádzka","dBA","19","","","","","","22"]
["","","","Nízka","dBA","27","","","","","","33"]
["","Chladenie","","Tichá prevádzka","dBA","19","","","","","","21"]
["","","","Nízka","dBA","24","","","","","","33"]
["","","","Vysoké","dBA","40","","","","","","45"]
["","","","Men.","dBA","34","","","","","","39"]
["","Chladenie","","Men.","dBA","32","","","","","","39"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","","","","","","1"]
["","Návod na prevádzku","","","","1","","","","","","1"]
["","Bezdrôtové diaľkové ovládanie","","","","1","","","","","","1"]
["","Batérie","","","","2","","","","","","2"]
["","Držiak diaľkového ovládača","","","","1","","","","","","1"]
["","Montážna platnička","","","","1","","","","","","1"]
["","Titánovo apatitový fotokatalytický filter na čistenie vzduchu","","","","2","","","","","","2"]
["","Upevňovacie skrutky vnútornej jednotky","","","","2","","","","","","2"]
["Riadiace systémy","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","","","","","","6.35"]
["","Plyn","","OD","mm","9.5","","","","","","9.5"]
["","Vypúšťanie","","","","18","","","","","","18"]
["Power input","Chladenie","","Men.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Kúrenie","","Men.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Chladenie","","","dBA","58","","","","","","59"]
["","Vykurovanie","","","dBA","58","","","","","","59"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","780","","","","","","900"]
["","","","Hĺbka","mm","215","","","","","","215"]
["","","","Výška","mm","289","","","","","","298"]
["Opláštenie","Farba","","","","Biela","","","","","","Biela"]
["Hmotnosť","Jednotka","","","kg","8","","","","","","11"]
["Power supply","Fáza","","","","1~","","","","","","1~"]
["","Frekvencia","","","Hz","50","","","","","","50"]
["","Názov","","","","V1","","","","","","V1"]
["","Napätie","","","V","220-240","","","","","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","","","","","","","(4) - 240 V"]
["Vstup napájania","Chladenie","","Men.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Kúrenie","","Men.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Opláštenie","Farba","","","","","Biela","Biela","Biela","Biela","Biela","","Biela","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","215","289","215","298","215","","215","298","215"]
["","","","Šírka","mm","","780","780","780","900","900","","900","900","900"]
["","","","Hĺbka","mm","","289","215","289","215","298","","298","215","298"]
["Hmotnosť","Jednotka","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Stredný","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Nízka","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Tichá prevádzka","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Kúrenie","Vysoké","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","Vykurovanie","Stredný","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Kúrenie","Nízka","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Tichá prevádzka","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Akustický výkon","Chladenie","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Vykurovanie","","","dBA","","58","58","58","59","59","","59","60","60"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Stredný","dBA","","32","33","33","","37","","39","","40"]
["","","","Nízka","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Tichá prevádzka","dBA","","19","19","19","19","19","","21","23","23"]
["","Kúrenie","","Vysoké","dBA","","40","41","41","45","45","","45","47","47"]
["","Vykurovanie","","Stredný","dBA","","34","34","34","","39","","39","","40"]
["","Kúrenie","","Nízka","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Tichá prevádzka","dBA","","19","19","19","19","19","","22","24","24"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Plyn","","OD","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Odvod kondenzátu","","","","","18","18","18","18","18","","18","18","18"]
["Riadiace systémy","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Štandardné príslušenstvo","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Napájanie","Názov","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fáza","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Napätie","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilátor","Prietok vzduchu","Chladenie","Men.","m³/min","","","9.1","","11.2","","","","11.9"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","","","33","","37","","","","40"]
["Ventilátor","Prietok vzduchu","Kúrenie","Men.","m³/min","","","8.0","","9.3","","","","10.8"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","","","34","","39","","","","40"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Štandardné príslušenstvo","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]