{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Hladina akustického tlaku","Kúrenie","Vysoké","dBA","41"]
["","","Stredný","dBA","31"]
["","","Tichá prevádzka","dBA","19"]
["","","Nízka","dBA","24"]
["","Chladenie","Stredný","dBA","32"]
["","","Tichá prevádzka","dBA","20"]
["","","Nízka","dBA","25"]
["","","Vysoké","dBA","43"]
["Štandardné príslušenstvo","Návod na montáž","","","1"]
["","Návod na prevádzku","","","1"]
["","Vzduchový filter","","","2"]
["","Infračervené diaľkové ovládanie","","","1"]
["","Montážna platnička diaľkového ovládača","","","1"]
["","Nádobka na skrutky","","","1"]
["","Kryt na skrutky","","","2"]
["","Batérie so suchými článkami typu AAA","","","2"]
["","Všeobecné bezpečnostné opatrenia","","","1"]
["Chladiace médium","GWP","","","675.0"]
["Riadiace systémy","Wired remote control","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Pripojenia potrubí","Kvapalina","OD","mm","6.35"]
["","Plyn","OD","mm","9.50"]
["","Vypúšťanie","","","18"]
["Príkon","Chladenie","Men.","kW","0.023"]
["","Kúrenie","Men.","kW","0.022"]
["Sound power level","Chladenie","","dBA","60"]
["","Vykurovanie","","dBA","60"]
["Vonkajšie rozmery","Jednotka","Šírka","mm","798"]
["","","Hĺbka","mm","189"]
["","","Výška","mm","295"]
["Opláštenie","Farba","","","Biela"]
["Hmotnosť","Jednotka","","kg","11.5"]
["Power supply","Fáza","","","1~"]
["","Frekvencia","","Hz","50"]
["","Názov","","","V1"]
["","Napätie","","V","220-240"]