{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Hladina akust. tlaku","Kúrenie","","Vysoké","dBA","41"]
["","","","Stredný","dBA","31"]
["","","","Tichá prevádzka","dBA","19"]
["","","","Nízka","dBA","24"]
["","Chladenie","","Medium","dBA","32"]
["","","","Tichá prevádzka","dBA","20"]
["","","","Nízka","dBA","25"]
["","","","Vysoké","dBA","43"]
["Štandardné príslušenstvo","Návod na montáž","","","","1"]
["","Návod na prevádzku","","","","1"]
["","Vzduchový filter","","","","2"]
["","Infračervené diaľkové ovládanie","","","","1"]
["","Montážna platnička diaľkového ovládača","","","","1"]
["","Nádobka na skrutky","","","","1"]
["","Kryt na skrutky","","","","2"]
["","Batérie so suchými článkami typu AAA","","","","2"]
["","Všeobecné bezpečnostné opatrenia","","","","1"]
["Chladiace médium","GWP","","","","675.0"]
["Riadiace systémy","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","18"]
["Vstup napájania","Chladenie","","Men.","kW","0.023"]
["","Kúrenie","","Men.","kW","0.022"]
["Úroveň akustického výkonu","Chladenie","","","dBA","60"]
["","Vykurovanie","","","dBA","60"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","798"]
["","","","Hĺbka","mm","189"]
["","","","Výška","mm","295"]
["Opláštenie","Colour","","","","Biela"]
["Hmotnosť","Unit","","","kg","11.5"]
["Fan","Prietok vzduchu","Kúrenie","Vysoké","m³/min","11.5"]
["","","","Nízka","m³/min","6.0"]
["","","","Medium","m³/min","8.0"]
["","","","Tichá prevádzka","m³/min","5.1"]
["","","Chladenie","Nízka","m³/min","5.7"]
["","","","Medium","m³/min","8.3"]
["","","","Vysoké","m³/min","11.9"]
["","","","Tichá prevádzka","m³/min","4.6"]
["Power supply","Fáza","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Názov","","","","V1"]
["","Voltage","","","V","220-240"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27 °CDB, 19,0 °CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch"]