{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB / RXTA-C"]
[]
[]
[]
[]
["","","","","FTXTA30C2V1BB / RXTA30C2V1B"]
["Chladiaci výkon","Min.","","kW","1.2"]
["","Men.","","kW","3"]
["","Max.","","kW","4.6"]
["Vykurovací výkon","Min.","","kW","0.8"]
["","Men.","","kW","3.2"]
["","Max.","","kW","7.1"]
["Nominálna účinnosť","EER","","","4.89"]
["","COP","","","5.01"]
["","Ročná spotreba energie","","kWh","307"]
["","Smernica o energetickom označovaní","Chladenie","","A"]
["","","Vykurovanie","","A"]
["Chladenie","Trieda energetickej účinnosti","","","A+++"]
["","Výkon","P návrh","kW","3"]
["","SEER","","","8.75"]
["","Ročná spotreba energie","","kWh/rok","120"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A+++"]
["","Výkon","P návrh","kW","3"]
["","SCOP/A","","","5.17"]
["","Pdh Vykurovací výkon pri -10°","","kW","3"]
["","Ročná spotreba energie","","kWh/rok","812"]
["Poznámky","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]