{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.029","0.053"]
["","Kúrenie","","Men.","kW","0.024","0.06"]
["Opláštenie","Farba","","","","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","298","298"]
["","","","Šírka","mm","804","997"]
["","","","Hĺbka","mm","252","292"]
["Hmotnosť","Jednotka","","","kg","12","15"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","13.2","15.1"]
["","","","Stredný","m³/min","8.1","9.2"]
["","","","Nízka","m³/min","5.6","5.6"]
["","","","Tichá prevádzka","m³/min","4.8","4.8"]
["","","Kúrenie","Vysoké","m³/min","11.7","17"]
["","","Vykurovanie","Stredný","m³/min","7.7","10"]
["","","Kúrenie","Nízka","m³/min","5.6","6"]
["","","","Tichá prevádzka","m³/min","4.7","5.1"]
["Akustický výkon","Chladenie","","","dBA","60","60"]
["","Vykurovanie","","","dBA","59","60"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","45","46"]
["","","","Stredný","dBA","33","32"]
["","","","Nízka","dBA","25","24"]
["","","","Tichá prevádzka","dBA","21","20"]
["","Kúrenie","","Vysoké","dBA","43","46"]
["","Vykurovanie","","Stredný","dBA","31","31"]
["","Kúrenie","","Nízka","dBA","22","22"]
["","","","Tichá prevádzka","dBA","19","19"]
["Chladivo","GWP","","","","675","675"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35"]
["","Plyn","","OD","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARC466A83","ARC466A83"]
["Štandardné príslušenstvo","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napájanie","Názov","","","","V1","V1"]
["","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","(3) - Elektrické údaje nájdete v samostatných nákresoch"]
["Štandardné príslušenstvo","FTXTM40A2V1B","","","","","1"]