{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M / RXTM-N"]
[]
[]
[]
[]
["","","","","FTXTM30M2V1B / RXTM30N2V1B","FTXTM40M2V1B / RXTM40N2V1B"]
["Chladiaci výkon","Min.","","kW","0.70","0.70"]
["","Max.","","kW","4.50","5.10"]
["","Men.","","kW","3.00","4.00"]
["Nominálna účinnosť","Annual energy consumption","","kWh","366","542"]
["","EER","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","A"]
["Vykurovací výkon","Men.","","kW","3.20","4.00"]
["","Min.","","kW","0.80","0.80"]
["","Max.","","kW","6.70","7.20"]
["Poznámky","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(2) - Chladenie: T2: vnút. tepl. 26,6°CDB, 19,4°CWB, vonk. tepl. 48°CDB [Btu/h/W]","(2) - Chladenie: T2: vnút. tepl. 26,6°CDB, 19,4°CWB, vonk. tepl. 48°CDB [Btu/h/W]"]
["","","","","(3) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(3) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]