{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.032","0.037"]
["","Kúrenie","","Men.","kW","0.037","0.04"]
["Opláštenie","Farba","","","","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","294","300"]
["","","","Šírka","mm","811","1040"]
["","","","Hĺbka","mm","272","295"]
["Hmotnosť","Jednotka","","","kg","10","14.5"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","11.7","15.5"]
["","","","Stredný","m³/min","8","9.2"]
["","","","Nízka","m³/min","6.3","5.7"]
["","","","Tichá prevádzka","m³/min","5.2","4.6"]
["","","Kúrenie","Vysoké","m³/min","12.2","17.7"]
["","","Vykurovanie","Stredný","m³/min","7.5","11"]
["","","Kúrenie","Nízka","m³/min","5.1","7.5"]
["","","","Tichá prevádzka","m³/min","4.1","6.3"]
["Akustický výkon","Chladenie","","","dBA","60","60"]
["","Vykurovanie","","","dBA","61","61"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","45","46"]
["","","","Stredný","dBA","33","32"]
["","","","Nízka","dBA","25","24"]
["","","","Tichá prevádzka","dBA","21","20"]
["","Kúrenie","","Vysoké","dBA","45","46"]
["","Vykurovanie","","Stredný","dBA","31","31"]
["","Kúrenie","","Nízka","dBA","22","22"]
["","","","Tichá prevádzka","dBA","19","19"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35"]
["","Plyn","","OD","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","16 (vnútorný priemer prepojovacej hadice)","16 (vnútorný priemer prepojovacej hadice)"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARC466A55","ARC466A55"]
["","Káblový diaľkový ovládač","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Napájanie","Názov","","","","V1","V1"]
["","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]