{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","45.0"]
["","","","Stredný","dBA","31.0"]
["","","","Tichá prevádzka","dBA","19.0"]
["","","","Nízka","dBA","22.0"]
["","Chladenie","","Medium","dBA","33.0"]
["","","","Tichá prevádzka","dBA","21.0"]
["","","","Nízka","dBA","25.0"]
["","","","Vysoké","dBA","45.0"]
["Štandardné príslušenstvo","Návod na montáž","","","","1"]
["","Návod na prevádzku","","","","1"]
["","Bezdrôtové diaľkové ovládanie","","","","1"]
["","Batérie so suchými článkami typu AAA","","","","2"]
["","Držiak diaľkového ovládača","","","","1"]
["","Montážna platnička","","","","1"]
["","Upevňovacie skrutky vnútornej jednotky","","","","2"]
["","Strieborný filter pevných častíc","","","","1"]
["Riadiace systémy","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Pripojenia potrubí","Liquid","","OD","mm","6.35"]
["","Plyn","","OD","mm","9.50"]
["","Vypúšťanie","","","","18"]
["Vstup napájania","Chladenie","","Men.","kW","0.035"]
["","Kúrenie","","Men.","kW","0.039"]
["Sound power level","Chladenie","","","dBA","60.0"]
["","Vykurovanie","","","dBA","61.0"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","778"]
["","","","Hĺbka","mm","272"]
["","","","Výška","mm","295"]
["Casing","Farba","","","","Biela"]
["Hmotnosť","Jednotka","","","kg","10.0"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","12.5"]
["","","","Nízka","m³/min","4.9"]
["","","","Medium","m³/min","7.5"]
["","","","Tichá prevádzka","m³/min","4.0"]
["","","Chladenie","Nízka","m³/min","5.3"]
["","","","Medium","m³/min","7.8"]
["","","","Vysoké","m³/min","12.2"]
["","","","Tichá prevádzka","m³/min","4.1"]
["Power supply","Fáza","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Názov","","","","V1"]
["","Napätie","","","V","220-240"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27 °CDB, 19,0 °CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["","","","","","(3) - Pozrite si samostatné nákresy s elektrickými údajmi"]
["Vstup napájania","Chladenie","","Men.","kW","","0.053"]
["","Kúrenie","","Men.","kW","","0.06"]
["Opláštenie","Farba","","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","299"]
["","","","Šírka","mm","","998"]
["","","","Hĺbka","mm","","292"]
["Hmotnosť","Jednotka","","","kg","","14.5"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","15.4"]
["","","","Stredný","m³/min","","9.5"]
["","","","Nízka","m³/min","","5.8"]
["","","","Tichá prevádzka","m³/min","","4.6"]
["","","Kúrenie","Vysoké","m³/min","","17.5"]
["","","Vykurovanie","Stredný","m³/min","","10.5"]
["","","Kúrenie","Nízka","m³/min","","7.1"]
["","","","Tichá prevádzka","m³/min","","5.9"]
["Akustický výkon","Chladenie","","","dBA","","60"]
["","Vykurovanie","","","dBA","","61"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","46"]
["","","","Stredný","dBA","","32"]
["","","","Nízka","dBA","","24"]
["","","","Tichá prevádzka","dBA","","20"]
["","Kúrenie","","Vysoké","dBA","","46"]
["","Vykurovanie","","Stredný","dBA","","31"]
["","Kúrenie","","Nízka","dBA","","22"]
["","","","Tichá prevádzka","dBA","","19"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","6.35"]
["","Plyn","","OD","mm","","9.5"]
["","Odvod kondenzátu","","","","","18"]
["Riadiace systémy","Infrared remote control","","","","","ARC466A75"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","","BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napájanie","Názov","","","","","V1"]
["","Fáza","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50"]
["","Napätie","","","V","","220-240"]