{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.032","0.032"]
["","Kúrenie","","Men.","kW","0.032","0.032"]
["Opláštenie","Farba","","","","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","286","286"]
["","","","Šírka","mm","770","770"]
["","","","Hĺbka","mm","225","225"]
["Hmotnosť","Jednotka","","","kg","9","9"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","11","11"]
["","","","Stredný","m³/min","7.9","7.9"]
["","","","Nízka","m³/min","5","5"]
["","","","Tichá prevádzka","m³/min","3.7","3.7"]
["","","Kúrenie","Vysoké","m³/min","10.5","10.5"]
["","","Vykurovanie","Stredný","m³/min","9","9"]
["","","Kúrenie","Nízka","m³/min","5.5","5.5"]
["","","","Tichá prevádzka","m³/min","4.4","4.4"]
["Akustický výkon","Chladenie","","","dBA","58","58"]
["","Vykurovanie","","","dBA","58","58"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","43","43"]
["","","","Stredný","dBA","35","35"]
["","","","Nízka","dBA","26","26"]
["","","","Tichá prevádzka","dBA","21","21"]
["","Kúrenie","","Vysoké","dBA","43","43"]
["","Vykurovanie","","Stredný","dBA","35","35"]
["","Kúrenie","","Nízka","dBA","26","26"]
["","","","Tichá prevádzka","dBA","21","21"]
["Chladivo","GWP","","","","675","675"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35"]
["","Plyn","","OD","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Štandardné príslušenstvo","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napájanie","Názov","","","","V1","V1"]
["","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35°CDB, 24°CWB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","(3) - Elektrické údaje nájdete v samostatných nákresoch"]
["Štandardné príslušenstvo","FTXTP35A5V1B","","","","","1"]