{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","43"]
["","","","Stredný","dBA","35"]
["","","","Tichá prevádzka","dBA","21"]
["","","","Nízka","dBA","26"]
["","Chladenie","","Stredný","dBA","35"]
["","","","Tichá prevádzka","dBA","21"]
["","","","Nízka","dBA","26"]
["","","","Vysoké","dBA","43"]
["Štandardné príslušenstvo","Návod na montáž","","","","1"]
["","Návod na prevádzku","","","","1"]
["","Bezdrôtové diaľkové ovládanie","","","","1"]
["","Batérie so suchými článkami typu AAA","","","","2"]
["","Držiak diaľkového ovládača","","","","1"]
["","Montážna platnička","","","","1"]
["","Deodorizačný titánium apatitový filter","","","","2"]
["","Upevňovacie skrutky vnútornej jednotky","","","","2"]
["Riadiace systémy","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Kvapalina","","OD","mm","6.35"]
["","Plyn","","OD","mm","9.50"]
["","Drain","","","","16 (vnútorný priemer prepojovacej hadice)"]
["Príkon","Chladenie","","Men.","kW","0.030"]
["","Kúrenie","","Men.","kW","0.035"]
["Úroveň akustického výkonu","Chladenie","","","dBA","58"]
["","Vykurovanie","","","dBA","58"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","770"]
["","","","Hĺbka","mm","225"]
["","","","Výška","mm","285"]
["Opláštenie","Colour","","","","Biela"]
["Hmotnosť","Jednotka","","","kg","9.0"]
["Power supply","Fáza","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Názov","","","","V1"]
["","Voltage","","","V","220-240"]
["Poznámky","","","","","(1) - Elektrické údaje nájdete v samostatných nákresoch"]
["Vstup napájania","Chladenie","","Men.","kW","","0.03"]
["","Kúrenie","","Men.","kW","","0.035"]
["Opláštenie","Farba","","","","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","285"]
["","","","Šírka","mm","","770"]
["","","","Hĺbka","mm","","225"]
["Hmotnosť","Jednotka","","","kg","","9"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","11.4"]
["","","","Stredný","m³/min","","8.2"]
["","","","Nízka","m³/min","","5.4"]
["","","","Tichá prevádzka","m³/min","","4.3"]
["","","Kúrenie","Vysoké","m³/min","","10.8"]
["","","Vykurovanie","Stredný","m³/min","","7.8"]
["","","Kúrenie","Nízka","m³/min","","5.8"]
["","","","Tichá prevádzka","m³/min","","4.9"]
["Akustický výkon","Chladenie","","","dBA","","58"]
["","Vykurovanie","","","dBA","","58"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","43"]
["","","","Stredný","dBA","","35"]
["","","","Nízka","dBA","","26"]
["","","","Tichá prevádzka","dBA","","21"]
["","Kúrenie","","Vysoké","dBA","","43"]
["","Vykurovanie","","Stredný","dBA","","35"]
["","Kúrenie","","Nízka","dBA","","26"]
["","","","Tichá prevádzka","dBA","","21"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","6.35"]
["","Plyn","","OD","mm","","9.5"]
["","Odvod kondenzátu","","","","","16 (vnútorný priemer prepojovacej hadice)"]
["Riadiace systémy","Infrared remote control","","","","","ARC480A11"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","","BRC944B2, BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napájanie","Názov","","","","","V1"]
["","Fáza","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50"]
["","Napätie","","","V","","220-240"]