{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZA-D"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / FUA100AVEB9 / RZA200D7Y1B","FUA71AVEB9 / FUA71AVEB9 / FUA71AVEB9 / RZA200D7Y1B","FUA125AVEB9 / FUA125AVEB9 / RZA250D7Y1B (Archived)"]
["Chladiaci výkon","Men.","","kW","19.0 (1)","19.0 (1)"]
["Chladenie priestoru","SEER","","","7.01","7.39"]
["","ηs, c","","%","278","292"]
["","Ročná spotreba energie","","kWh/a","1,625","1,543"]
["","Výkon","P návrh","kW","19.0","19.0"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","11.2","11.2"]
["","SCOP/A","","","4.10","4.15"]
["","Ročná spotreba energie","","kWh/a","3,825","3,779"]
["","ηs, h","","%","161","163"]
["Vykurovací výkon","Men.","","kW","22.4 (2)","22.4 (2)"]
["Poznámky","","","","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Chladiaci výkon","Men.","","kW","","","22.0 (1)"]
["Vykurovací výkon","Men.","","kW","","","24.0 (2)"]
["Chladenie","Výkon","P návrh","kW","","","22.0"]
["","SEER","","","","","6.10"]
["","Ročná spotreba energie","","kWh/a","","","2163"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","","12.1"]
["","SCOP/A","","","","","4.10"]
["","Ročná spotreba energie","","kWh/a","","","4132"]