{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / RZASG100M7Y1B","FUA125AVEB9 / RZASG125M7Y1B","FUA71AVEB9 / FUA71AVEB9 / RZASG140M7Y1B"]
["Chladiaci výkon","Men.","","kW","9.5","12.1","13.4"]
["Vykurovací výkon","Men.","","kW","10.8","13.5","15.5"]
["Chladenie","Trieda energetickej účinnosti","","","A+"]
["","Výkon","P návrh","kW","9.5","12.1","13.4"]
["","SEER","","","5.83","5.49","8.56"]
["","Ročná spotreba energie","","kWh/rok","570","1322","939"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A+"]
["","Výkon","P návrh","kW","6","6","7.80"]
["","SCOP/A","","","4.01","3.84","5.00"]
["","Ročná spotreba energie","","kWh/rok","2095","2188","2185"]
["Rozsah energetickej účinnosti","","","","","","A+++ ~ D"]
["Poznámky","","","","","","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]